Text for specification

Описание 
Перфорированный
230 x 1100
60Classic

Стандарты
IEC 61439-1:2011

Электрические данные

Свойства материала
Cover:
	temperature stability 70°C, 
	self-extinguishing in acc. to UL 94

Miscellaneous 
To safeguard against touching the busbars from above, below and behind, with slotted sections that can be punched out to pass leads through.

Brand 
Woehner or equivalent

Арт.
01009000