Text for specification

Описание 
CRITO^®
Универсальная клемма
16 - 70 mm², AWG 6 - 2/0
30Compact 3P
60Classic

Стандарты
IEC 61439-1:2011
IEC 60999-1:1999
IEC 60999-2:2003

Сертификация
CSA, UL

Электрические данные
Номинальный ток (IEC):	175 A
номинальное напряжение (IEC) AC:	690 В

номинальный ток (UL):	175 A
номинальное напряжение (UL) AC:	600 В
токовая нагрузка (IEC) макс.:	400 A
макс. напряжение IEC AC:	1000 В
макс. напряжение IEC DC:	1500 В

номинальный выдерживаемый пиковый ток I  _pk  макс.:	46,7 кА

Особенности клеммной техники
16 - 70 mm² / AWG 4 - AWG 2/0 
flexible cables, directly or with wire-end ferrule, 
solid round cables, 
lam. Cu 2x 3 x 9 x 0.8 or 6 x 9 x 0.8 or 6 x 13 x 0.5

(flexible cables of maximum cross-section may not fit when using wire-end ferrule)

Свойства материала
Connecting screws:
	hexagon head cap screw M8
	length across flats 13
	galvanized, chromized
Terminal body:
	steel, galvanized and chromized
Retaining spring:
	corrosion-resistant spring steel

Miscellaneous 
Terminal with integrated holding spring, captive clamping screw and opened terminal space.
Indication of nominal cross-section and tightening torque noted on the terminal.

Brand 
Woehner or equivalent

Арт.
01287000