Text for specification

Описание 
CRITO®
Цанговая клемма
lam. Cu. 20x3 ... 32x15
60Classic
100Energy
185mm-System
Центральный ввод питания

Стандарты
IEC 61439-1:2011
IEC 60999-1:1999
IEC 60999-2:2003

Сертификация
UL

Электрические данные
Номинальный ток (IEC):	500 A
номинальное напряжение (IEC) AC:	690 В

номинальный ток (UL):	800 A
номинальное напряжение (UL) AC:	600 В
Допустимая нагрузка по току при центральном вводе питания:	750 A
токовая нагрузка (IEC) макс.:	750 A
макс. напряжение IEC AC:	1000 В
макс. напряжение IEC DC:	1500 В

SCCR:	25 кА

Особенности клеммной техники
lam. Cu from 3 x 20 x 1 to 10 x 24 x 1

Свойства материала
Connecting screws:
	Set screw M16, Allan key size 8
Terminal body:
	steel, galvanized and chromized
cable base:
	brass, tin plated

Terminal body: 	galvanised steel, chromited screw: 	hexagonal socket screw M16 x 1.5 (S8), galvanised, chromited

Miscellaneous 
Terminal with captive clamping screws, conductor can be overlapped, indication of nominal cross-section and tightening torque noted on the terminal. Contact between conductor and busbar via contact block.

Brand 
Woehner or equivalent

Арт.
01319000