Text for specification

Описание 
AMBUS^®Panel
Держатель цилиндрических предохранителей
10 x 38 / 1P/N
32 A / 690 В, с Нейтралью

Стандарты
IEC 60947-1:2020
IEC 60947-3:2020 AC ratings only

Сертификация
CCC

Электрические данные
Номинальный ток (IEC):	32 A
номинальное напряжение (IEC) AC:	690 В

рассеиваемая мощность при номинальном непрерывном токе устройства:	0,9 Вт

номинальное напряжение изоляции U  _i  AC:	690 В
номинальное импульсное напряжение U  _imp :	4 kV
макс. напряжение IEC AC:	725 В

for fuse links as per IEC / EN 60269-2
with permitted rated power dissipations
up to max. 3W for gG/gL
up to max. 1.2W for aM

Свойства материала
Main body:
	temperature stability 125°C, 
	self-extinguishing in acc. to UL 94, 
	creepage resistance CTI 600,
	halogen-free
Fuse-carrier:
	temperature stability 125°C, 
	self-extinguishing in acc. to UL 94, 
	creepage resistance CTI 600,
	halogen-free
	
Connecting screws:
	screw +/- (PZ2), galvanized, chromized 

Miscellaneous 
large clamping range
holder for label

Brand 
Woehner or equivalent

Арт.
31273000A