Text for specification

Описание 
TRITON®Panel
Держатель D0-предохранителей, панельный монтаж
E 14 / 16 A / 1P
С защитой от прикосновения в соотв. с DGUV V3

Стандарты
IEC 60269-1:2006 + A1:2009 + A2:2014
IEC 60269-3:2010 + A1:2013 + A2:2019

Сертификация
CCC

Электрические данные
Номинальный ток (IEC):	16 A
номинальное напряжение (IEC) AC:	400 В
номинальное напряжение (IEC) DC:	250 В

рассеиваемая мощность при номинальном непрерывном токе устройства:	0,4 Вт
номинальное импульсное напряжение U  imp :	6 kV
макс. напряжение IEC AC:	440 В
макс. напряжение IEC DC:	262 В
устойчивость к короткому замыканию при защите предохранителями:	50 кА

Особенности клеммной техники
box terminal :
1,5 - 35 mm² flexible cables, directly or with wire-end ferrule,
1,5 - 10 mm² solid round cables
Md 4,0 Nm

(flexible cables of maximum cross-section may not fit when using wire-end ferrule)

Свойства материала
Body:
	temperature stability 125°C, 
	self-extinguishing in acc. to UL 94, 
	creepage resistance CTI 600,
	halogen-free
Connecting screws:
	screw +/- (PZ2), galvanized, chromized 

Miscellaneous 
large clamping range, holder for label

Brand 
Woehner or equivalent

Арт.
31286000