Text for specification

Описание 
QUADRON^®100Energy
Линейный держатель NH предохранителей, 160 A
Зажимная клемма 70 мм²
Типоразмер 00
100Energy

Стандарты
IEC 60269-1:2006 + A1:2009 + A2:2014
IEC 60269-2:2013 + A1:2016

Электрические данные
Номинальный ток (IEC):	160 A
номинальное напряжение (IEC) AC:	690 В

рассеиваемая мощность при номинальном непрерывном токе устройства:	17,5 Вт
номинальное импульсное напряжение U  _imp :	6 kV
макс. напряжение IEC AC:	800 В
устойчивость к короткому замыканию при защите предохранителями:	50 кА

Особенности клеммной техники
wedge clamp terminal for Cu an Al:
stranded round 16 - 70 mm²,
stranded sectored 16 - 70 mm²,
flexible with wire-end ferrules 16 - 70 mm²

(flexible cables of maximum cross-section may not fit when using wire-end ferrule)

Свойства материала
Main body:
	temperature stability 125°C, 
	self-extinguishing in acc. to UL 94, 
	creepage resistance CTI 200
Contacts:
	spring-loaded copper contacts, silver plated 
Shock protection cover:
	temperature stability 125°C, 
	self-extinguishing in acc. to UL 94, 
	creepage resistance CTI 600,
	halogen-free

Miscellaneous 
Undrilled mounting possible with terminal clamp

Brand 
Woehner or equivalent

Арт.
33384000