Text for specification

Описание 
AMBUS®Panel
Держатель цилиндрических предохранителей, с контрольным доп. контактом
14 x 51 / 1P
50 A / 690 V

Стандарты
IEC 60947-1:2020
IEC 60947-3:2020 AC ratings only

Сертификация
CSA, UL, CCC

Электрические данные
Номинальный ток (IEC):	50 A
номинальное напряжение (IEC) AC:	690 В

номинальный ток (UL):	50 A
номинальное напряжение (UL) AC:	600 В
номинальное напряжение (UL) DC:	600 В

рассеиваемая мощность при номинальном непрерывном токе устройства:	0,9 Вт

номинальное напряжение изоляции U  i  AC:	800 В
номинальное импульсное напряжение U  imp :	6 kV

SCCR:	100 кА

for fuse links with striker as per IEC / EN 60269-2 with permitted rated power dissipationsup to max. 5W for gG/gL up to max. 3W for aMup to max. 6.5W for aR/gR at max. 40A pilot switch1 changeover switch 250V AC (5A), 30V DC (4A)

Особенности клеммной техники
box terminal :
1,5 - 35 mm² / AWG 14 - AWG 2 
flexible cables, directly or with wire-end ferrule
Md 2,5 - 3,0 Nm / 22 - 26 lb.in.

(flexible cables of maximum cross-section may not fit when using wire-end ferrule)

Miscellaneous 
large clamping range
 holder for label

Brand 
Woehner or equivalent

Арт.
31940000