Text for specification

Описание 
CRITO®60Classic
Подсоединительная клеммная платформа, 3-полюсная
6 - 50 mm², AWG 10 - 2/0, lam. Cu. 7 - 9 x 4 - 10
60Classic

Стандарты
IEC 61439-1:2011
IEC 60999-1:1999
IEC 60999-2:2003

Сертификация
CSA, UL

Электрические данные
Номинальный ток (IEC):	175 A
номинальное напряжение (IEC) AC:	800 В

номинальный ток (UL):	175 A
номинальное напряжение (UL) AC:	600 В

рассеиваемая мощность при номинальном непрерывном токе устройства:	3,0 Вт
токовая нагрузка (IEC) макс.:	300 A
номинальное импульсное напряжение U  imp :	6 kV
макс. напряжение IEC AC:	1000 В
макс. напряжение IEC DC:	1500 В

номинальный выдерживаемый пиковый ток I  pk  макс.:	40,5 кА

SCCR: 65 kA with any DIVQ/7 circuit breaker 200 A / 480 V AC, 100 kA with JDDZ fuse Class J, CF or T 150 A / 600 V AC 

Особенности клеммной техники
6 - 50 (70) mm² / AWG 10 - AWG 2/0 
flexible cables, directly or with wire-end ferrule, 
stranded round cables 
lam. Cu 7x4 - 9x6
Md 8-10 Nm / 71 lb-in

(flexible cables of maximum cross-section may not fit when using wire-end ferrule)

Свойства материала
Main body:
	temperature stability 125°C, 
	self-extinguishing in acc. to UL 94, 
	creepage resistance CTI 200,
	halogen-free
Cover:
	temperature stability 125°C, 
	self-extinguishing in acc. to UL 94, 
	creepage resistance CTI 200,
	halogen-free

Miscellaneous 
Terminals can be removed for connection of uncut conductors

Brand 
Woehner or equivalent

Арт.
01240000