Text for specification

Описание 
EQUES^®30Compact
шинный адаптер 30 A
для прямого пускателя Siemens S0 с пружинным подсоединением
45 x 160, с проводами AWG 10 (6 мм²)
30Compact 3P

Стандарты
IEC 61439-1:2011

Сертификация
CSA, UL

Электрические данные
Номинальный ток (IEC):	30 A
номинальное напряжение (IEC) AC:	690 В

номинальный ток (UL):	30 A
номинальное напряжение (UL) AC:	600 В

рассеиваемая мощность при номинальном непрерывном токе устройства:	2,5 Вт

номинальное напряжение изоляции U  _i  AC:	800 В
номинальное импульсное напряжение U  _imp :	6 kV

SCCR: 65 kA with any NKJH Comb. Motor Controller 16 A / 480 V AC, 65 kA with any NKJH Comb. Motor Controller 25 A / 480 V AC, 30 kA with any NKJH Comb. Motor Controller 12,5 A / 600 V AC, 50 kA with any NKJH Comb. Motor Controller 32 A / 480 V AC 

Свойства материала
Conductor insulation: 	temperature-resistant up to 105 °C

Miscellaneous 
Conductor ends ultrasonically sealed.
Click mechanism when pushing onto the busbar.

Brand 
Woehner or equivalent

Арт.
32694000A