Text for specification

Описание 
EQUES 185Power
Шинный адаптер 1250 A
300 x 652, подсоединение сверху, зажим хомутом
185Power

The 185Power is an innovative busbar system for energy distribution coming with busbar system, connection rails and modules as feeders, busbar connectors, NH in-line fuse-switch-disconnectors, NH switch-disconnector-fuses and adapters for circuit breakers.

 By using Crosslink touch-safe protection modules, it is possible to build a touch-protected 185mm busbar system.

 Crosslink touch-safe protection cover with protection class IP2X front.
 Crosslink touch-safe protection cover with additional front cover enhance protection class to IP4X front.

 All system components can be mounted safely, easily and quickly on the Crosslink touch-safe protection modules using terminal clamps.

The busbar system comes with copper busbars of 30mm, 40mm, 60mm, 80mm, 100mm, 120mm x 10mm. For selected application set up’s, short circuit capabilities are proven by tests. The achievable maximum ratings are rated peak withstand current Ipk max. 105kA, rated short-time withstand current Icw max. 50kA at 1 second. 

Стандарты
IEC 61439-1:2020

Сертификация
UL

Электрические данные
Номинальный ток (IEC):	1 250 A
номинальное напряжение (IEC) AC:	800 В
номинальное напряжение (IEC) DC:	800 В

номинальный ток (UL):	1 200 A
номинальное напряжение (UL) AC:	1000 В

рассеиваемая мощность при номинальном непрерывном токе устройства:	363,0 Вт

номинальное напряжение изоляции U  i  AC:	1000 В
номинальное импульсное напряжение U  imp :	12 kV

номинальный выдерживаемый пиковый ток I  pk  макс.:	106 кА

Brand 
Woehner or equivalent

Арт.
32757000A