Text for specification

Описание 
Линейный выключатель-разъединитель с предохранителями 160 A
Винт M8 / зажим 70 мм², с электронным контролем состояния предохранителя
Типоразмер 00
100Energy
185mm-System

Стандарты
IEC 60947-1:2020
IEC 60947-3:2020 AC ratings only

Сертификация
IEC (CB), CCC

Электрические данные
Номинальный ток (IEC):	160 A
номинальное напряжение (IEC) AC:	400 В

AC-23B (400V)

рассеиваемая мощность при номинальном непрерывном токе устройства:	20,0 Вт

номинальное напряжение изоляции U  i  AC:	400 В
номинальное импульсное напряжение U  imp :	4 kV

Electronic fuse monitoring:
nominal voltage: 3AC 400V,
nominal frequency: 50...40Hz,
switch contact: 2 changeover switches, max. AC 250V, AC15  closer 3A, opener 1A,
rated surge voltage: 4kV,
pollution degree: 2

Degree of protection IP30 at front, degree of protection near terminal depends on installation

Особенности клеммной техники
screw M8 : 
Md 12 - 14 Nm

Miscellaneous 
Self-closing inspection holes are available in the cover.
Electronic fuse monitoring:
operating current principle, optionally with latching properties (latches without bridge X1-X2)
device display:
green LED = intact fuses
red LED = fuse tripped, cover position up

Brand 
Woehner or equivalent

Арт.
33286000