招标说明

说明
SECUR^®Panel
隔离开关熔断器组
3 极

标准
IEC 60947-1:2020
IEC 60947-3:2020 AC ratings only

认证许可
VDE, CCC

电气数值
额定电流（IEC）:	63 A
额定电压（IEC）AC:	400 V
额定电压 （IEC） DC:	130 V

AC-22B

power dissipation at full load of the item:	7.8 W

rated isolation voltage U_i AC:	500 V
额定冲击耐受电压 U_imp:	6 kV

for fuse links and gauge rings as per DIN VDE 0636-3 IEC / HD 60269-3
utilisation category as per VDE 0638 : AC-22

The function of isolation between incoming and outgoing contacts is provided by the opening of the switching mechanism as required in the standard.

连接端
框端子 : 
1.5 - 35 mm²    细密导线, 直接连接或通过导线套连接
(细密导线+导线套可能未达到最大横横截面积) 
1.5 - 10 mm²   单股导线
Md 2.5 - 3 Nm

如果框端子的两个接线室同时使用, 可以连接2条导线
最大可能的组合为35 mm² + 16 mm²

其他
双功能端子
任意的进线方向
不脱落的熔断器架
可铅封的手柄

品牌
维纳尔或同等价值的产品

订货号
31314000A