招标说明

说明
SECUR®Panel
隔离开关熔断器组
3 极 + N

标准
IEC 60947-1:2020
IEC 60947-3:2020 AC ratings only

认证许可
VDE, CCC

电气数值
额定电流（IEC）:	63 A
额定电压（IEC）AC:	400 V
额定电压 （IEC） DC:	130 V

AC-22B

power dissipation at full load of the item:	9.0 W

rated isolation voltage Ui AC:	500 V
额定冲击耐受电压 Uimp:	6 kV

for fuse links and gauge rings as per DIN VDE 0636-3 IEC / HD 60269-3
utilisation category as per VDE 0638 : AC-22

The function of isolation between incoming and outgoing contacts is provided by the opening of the switching mechanism as required in the standard.

其他
双功能端子
任意的进线方向
不脱落的熔断器架
可铅封的手柄

品牌
维纳尔或同等价值的产品

订货号
31315000A