Text for specification

Description
module PE/N
attachable to busbar adapter on both sides
18 x 242
60Classic

Standards
IEC 61439-1:2011

Approvals
UL

Electrical data
rated voltage (IEC) AC:	690 V

power dissipation at full load of the item:	1,4 W

rated isolation voltage U_i AC:	690 V

Connecting terminals 16 mm² top and bottom

Brand 
Woehner or equivalent

Part No.
32146000