Text for specification

Description
EQUES^®30Compact
busbar adapter 144 A, 3-pole
76 x 160
30Compact 3P

Standards
IEC 61439-1:2011

Electrical data
Rated current (IEC):	144 A
rated voltage (IEC) AC:	690 V

power dissipation at full load of the item:	12,0 W

rated isolation voltage U_i AC:	800 V
rated surge voltage U_imp :	6 kV

Brand 
Woehner or equivalent

Part No.
32661000A