Text for specification

Description
compartment section
slotted
17 x 86 x 1100
60Classic

Standards
IEC 61439-1:2011

Electrical data

Material properties
Cover:
	temperature stability 70°C, 
	self-extinguishing in acc. to UL 94

Miscellaneous 
To safeguard against touching the busbars from above and below, with slotted sections that can be punched out to pass leads through.

Brand 
Woehner or equivalent

Part No.
01041000