Text for specification

Description
lead AWG 10 (6 mm²), 190 mm long

Standards
IEC 61439-1:2020

Approvals
UL

Electrical data
power dissipation at full load of the item:	0.4 W

Brand 
Woehner or equivalent

Part No.
32935000A