Text for specification

Description
double-lead 2x AWG 10 (2x 6 mm²), 130 / 280 mm long
60Classic

Standards
IEC 61439-1:2020

Approvals
UL

Electrical data
power dissipation at full load of the item:	2.7 W

Brand 
Woehner or equivalent

Part No.
32915000