Text for specification

Description
CRITO^®
connection terminal for PE/N bar
35 mm²
suitable for PE and N busbars 01126 - 01130
Accessories

Standards
IEC 61439-1:2011
IEC 60999-1:1999
IEC 60999-2:2003

Electrical data
rated voltage (IEC) AC:	400 V
max. permitted voltage (IEC) AC:	500 V

Terminal points
1.5 - 25mm² flexible with wire-end ferrule
1.5 - 10mm² solid round 
only for maximum tightening torque:
16mm² stranded round

Brand 
Woehner or equivalent

Part No.
01114000