Text for specification

Description
cylindr. fuse link 25 A
690 V, gG
14 x 51
Accessories

Standards
IEC 60269-1:2006 + A1:2009 + A2:2014
IEC 60269-2:2013 + A1:2016, Fuse system F

Electrical data
Rated current (IEC):	25 A
rated voltage (IEC) AC:	690 V

power dissipation at full load of the item:	3.5 W

rated short-circuit breaking capacity AC:	80 kA

Brand 
Woehner or equivalent

Part No.
31193000