Text for specification

Description
CrossLink®30Compact
busbar adapter base 125 A
spare part
49.5 mm x 160 mm, only for use with QU-NH000
30Compact 3P

Standards
IEC 61439-1:2011

Electrical data
Rated current (IEC):	125 A
rated voltage (IEC) AC:	690 V

power dissipation at full load of the item:	4.0 W

rated isolation voltage Ui AC:	800 V
rated surge voltage Uimp :	6 kV

Brand 
Woehner or equivalent

Part No.
32619000A