Text for specification

Description
CRITO 60Classic
connection terminal plate, 3-pole
95 -  300 mm²
60Classic

Standards
IEC 61439-1:2020
IEC 60999-1:1999
IEC 60999-2:2003

Electrical data
rated current (IEC):	500 A
rated voltage (IEC) AC:	690 V
current capacity (IEC) max. of the terminal:	560 A
max. permitted voltage (IEC) AC:	1000 V
max. permitted voltage (IEC) DC:	1500 V

rated peak withstand current  Ipk max.:	63.1 kA

Miscellaneous 
Terminals with captive clamping screws
Conductor can be overlapped
Indication of nominal cross-section and tightening torque noted on the terminals.

Brand 
Woehner or equivalent

Part No.
01754000