Text for specification

Description
connecting latch with brace terminal
for screw conncetion M10 or M12
for cables Cu and Al 120 - 300 mm²
Accessories

Standards
IEC 61439-1:2011
IEC 60999-1:1999
IEC 60999-2:2003

Electrical data
Rated current (IEC):	600 A
rated voltage (IEC) AC:	690 V
max. permitted voltage (IEC) AC:	1000 V
max. permitted voltage (IEC) DC:	1500 V

Miscellaneous 
terminal embraces the cable
tightening torque is given at the terminal
rated cross-section is given at the connection latch     

Brand 
Woehner or equivalent

Part No.
01890000