Text for specification

Description
NH fuse 125 A
400 V, gG
size 000
Accessories

Standards
IEC 60269-1:2006 + A1:2009 + A2:2014
IEC 60269-2:2013 + A1:2016

Electrical data
Rated current (IEC):	125 A
rated voltage (IEC) AC:	400 V
rated voltage (IEC) DC:	250 V

power dissipation at full load of the item:	6.8 W

rated short-circuit breaking capacity AC:	120 kA
rated short-circuit breaking capacity DC:	25 kA

Brand 
Woehner or equivalent

Part No.
03243000