Text for specification

Description
busbar component support 1-pole
1 fixed mounting rail
18 x 160, without electrical connection
30Compact 5P

Standards
IEC 61439-1:2011

Electrical data
rated voltage (IEC) AC:	690 V

rated isolation voltage U_i AC:	800 V
rated surge voltage U_imp :	6 kV

Brand 
Woehner or equivalent

Part No.
32631000