Text for specification

Description
cover section
top / bottom, 1.10 m long, for holders 01136 or 01137
3 x 109 x 1100
60Classic

Standards
IEC 61439-1:2011
IEC 60999-1:1999
IEC 60999-2:2003

Approvals
CSA, UL

Electrical data

Material properties
Main body:
	temperature stability 70°C, 
	self-extinguishing in acc. to UL 94

Cover: temperature-resistant up to 75°C, self-releasing to UL 94, creepage current strength CTI 200, halogen-free

Brand 
Woehner or equivalent

Part No.
01555000