Text for specification

Description
insulator
with female thread at both sides, length across flats 40
M10 x 60
Accessories

Standards
IEC 61439-1:2011

Electrical data
rated voltage (IEC) AC:	3000 V
rated voltage (IEC) DC:	3000 V

Material properties
Main body:
	temperature stability 200°C, 
	self-extinguishing in acc. to UL 94, 
	creepage resistance CTI 600, 
	halogen-free

Brand 
Woehner or equivalent

Part No.
05789000