Text for specification

Description
EQUES®60Classic
busbar adapter 400 A, 4-pole
185 x 300
60Classic

Standards
IEC 61439-1:2011

Approvals
CSA, UL

Electrical data
Rated current (IEC):	400 A
rated voltage (IEC) AC:	690 V

rated current (UL):	630 A
rated voltage (UL) AC:	600 V

rated isolation voltage Ui AC:	800 V
rated surge voltage Uimp :	6 kV

Brand 
Woehner or equivalent

Part No.
32579000