Text for specification

Description
barrier for handle
for NH fuse-switch disconnector size 1-3
for closing of handle area from rear
60Classic

Standards
IEC 60947-1:2020
IEC 60947-3:2020 AC ratings only

Electrical data

Material properties
Main body:
	temperature stability 125°C, 
	self-extinguishing in acc. to UL 94, 
	creepage resistance CTI 200,
	halogen-free

Brand 
Woehner or equivalent

Part No.
33155000