Text for specification

Description
lid interlock
for sealing wire or 3 padlocks with shackle of 4 - 7 mm
Size 1 - 3
60Classic

Standards
IEC 60947-1:2020
IEC 60947-3:2020 AC ratings only

Electrical data

Brand 
Woehner or equivalent

Part No.
33157000