Text for specification

Description
busbar terminal for longitudinal connection
for cables
150 - 300 mm²
60Classic

Standards
IEC 61439-1:2011
IEC 60999-1:1999
IEC 60999-2:2003

Electrical data
rated voltage (IEC) AC:	690 V
max. permitted voltage (IEC) AC:	1000 V
max. permitted voltage (IEC) DC:	1500 V

Brand 
Woehner or equivalent

Part No.
01202000