Text for specification

Description
connection terminal, side connection
6 - 25 mm²
Accessories

Standards
IEC 61439-1:2011

Electrical data
Rated current (IEC):	80 A
rated voltage (IEC) AC:	690 V
rated surge voltage Uimp :	4 kV
max. permitted voltage (IEC) AC:	690 V
max. permitted voltage (IEC) DC:	1000 V

Terminal points
6 - 25 mm² round, solid and stranded
4 - 16 mm² flexible with wire-end ferrule
Md 2.5 Nm
max. connection diameter 6.5 mm

Brand 
Woehner or equivalent

Part No.
31103000