Text for specification

Description
lead AWG 8 (10 mm²), 190 mm long

Standards
IEC 61439-1:2011

Approvals
UL

Electrical data
power dissipation at full load of the item:	0.4 W

Brand 
Woehner or equivalent

Part No.
32936000A