Text for specification

Description
neutral conductor 63 A, disconnectable
socket terminal screw-on / snap-on

Standards
IEC 61439-1:2011

Electrical data
Rated current (IEC):	63 A
rated voltage (IEC) AC:	400 V
rated voltage (IEC) DC:	400 V

power dissipation at full load of the item:	0,2 W

Terminal points
16 mm²
2,5 - 3,0 Nm

Brand 
Woehner or equivalent

Part No.
05188000