Text for specification

Description
busbar support 1-pole, lateral
for section busbars
centre feed unit

Standards
IEC 61439-1:2011

Electrical data
rated voltage (IEC) AC:	690 V

rated isolation voltage U_i AC:	1000 V
rated surge voltage U_imp :	8 kV
max. permitted voltage (IEC) DC:	1500 V

7.5mm insulation between busbar and fixing plate

Brand 
Woehner or equivalent

Part No.
01369000