Text for specification

Description
touch-safe protection shroud for longitudinal connectors
3-pole, front and rear mounting, cover width 115 mm
mounting to 2 busbar supports 01430 with a center distance of 100 mm
185Power

Standards
IEC 61439-1:2020
IEC 60999-1:1999
IEC 60999-2:2003

Approvals
UL

Electrical data

Material properties
Main body:
	temperature stability 125°C, 
	self-extinguishing in acc. to UL 94, 
	creepage resistance CTI 200,
	halogen-free

Brand 
Woehner or equivalent

Part No.
01482000A