Text for specification

Description
EQUES®30Compact
busbar adapter 1-pole, 63 A
1 fixed mounting rail, for Schneider Electric iC60, iC65 and C60
18 x 160
30Compact 5P

Standards
IEC 61439-1:2011

Electrical data
Rated current (IEC):	63 A
rated voltage (IEC) AC:	690 V

power dissipation at full load of the item:	1.8 W

rated isolation voltage Ui AC:	800 V
rated surge voltage Uimp :	6 kV

Brand 
Woehner or equivalent

Part No.
32628000