Text for specification

Description
clip-on screw connection, for cable lugs
M8
60Classic
100Energy
185mm-System
centre feed unit

Standards
IEC 61439-1:2020

Electrical data
rated voltage (IEC) AC:	690 V

power dissipation at full load of the item:	0,5 W
current capacity (IEC) max. of the terminal:	490 A
max. permitted voltage (IEC) AC:	1000 V
max. permitted voltage (IEC) DC:	1500 V

rated peak withstand current  Ipk max.:	35,5 kA

Brand 
Woehner or equivalent

Part No.
01748000