Text for specification

Description
busbar support
1-pole, attachable to 01603 or individual mounting, with integrated end cover
60Classic

Standards
IEC 61439-1:2020

Electrical data
rated voltage (IEC) AC:	690 V

rated isolation voltage Ui AC:	1000 V
rated surge voltage Uimp :	8 kV
max. permitted voltage (IEC) DC:	1500 V

Tightening torque of the screws: 4 Nm

rated volteage (IEC) AC: 1000 V at pollution degree 2 and material class III

Brand 
Woehner or equivalent

Part No.
01355000