Text for specification

Description
busbar 30 x 5
length 2.40 m, tinned
60Classic

Standards
IEC 61439-1:2011

Approvals
CSA, UL

Electrical data
power dissipation at full load of the item:	64.0 W

Miscellaneous 
Tin-plated Cu busbars considerably reduce the effort of preparing the contact points.
The Cu busbars are effective protected against aggressive media.

Brand 
Woehner or equivalent

Part No.
01622000