Text for specification

Description
door coupling rotary drive
Accessories

Standards
IEC 60947-1:2020
IEC 60947-3:2020 AC ratings only

Approvals
UL

Electrical data

Miscellaneous 
lockable in 0-position with 3 padlocks (max. 6 mm diameter) door interlock in I-position door interlock in I-position defeatable with a tool 

Brand 
Woehner or equivalent

Part No.
33669000A