Text for specification

Description
component support
without electrical connection, 1 adjustable mounting rail
45 x 160

Standards
IEC 61439-1:2011

Approvals
IEC (CB), UL

Electrical data
rated voltage (IEC) AC:	690 V
rated voltage (UL) AC:	600 V

rated isolation voltage U_i AC:	800 V
rated surge voltage U_imp :	6 kV

Brand 
Woehner or equivalent

Part No.
32665000A