Text for specification

Description
current transformer 1000 A / 5 A
5 VA / class 1
185Power

Standards
IEC 61869-1:2007
IEC 61869-2:2012

Electrical data
power dissipation at full load of the item:	2,5 W

Material properties
Material: polyamide
electro casting resin
temperature-resistant up to 120 °C

Brand 
Woehner or equivalent

Part No.
32985000