Text for specification

Description
current transformer 910 A / 5 A
2.5 VA / class 0.5
when used on busbars or in 630 A adapters, 37900 is additionally required
Accessories

Standards
IEC 61869-1:2007
IEC 61869-2:2012

Electrical data
power dissipation at full load of the item:	6,8 W

Brand 
Woehner or equivalent

Part No.
37225000A