Text for specification

Description
cylindr. fuse link 20 A
1000 V DC, gPV
10 x 38
Accessories

Standards
IEC 60269-1:2006 + A1:2009 + A2:2014
IEC 60269-6:2010 + A1:2018

Electrical data
Rated current (IEC):	20 A
rated voltage (IEC) DC:	1000 V

power dissipation at full load of the item:	2.5 W
rated short-circuit breaking capacity DC:	30 kA

Brand 
Woehner or equivalent

Part No.
31547000