Text for specification

Description
flexible copper busbar, tinned, insulated
2x 15.5 x 0.8
200 A, length 3 m
Accessories

Standards
IEC 61439-1:2011

Approvals
UL

Electrical data

Miscellaneous 
Tin-plated Cu bars considerably reduce the effort of preparing the contact points.
The Cu busbars are effectively protected against aggressive media.

Brand 
Woehner or equivalent

Part No.
01523100