Text for specification

Descripción
perfil de separación
ranurado
17 x 86 x 1100
60Classic

Normas
IEC 61439-1:2011

datos eléctricos

Miscellaneous 
To safeguard against touching the busbars from above and below, with slotted sections that can be punched out to pass leads through.

Brand 
Woehner or equivalent

Part No.
01041000