Text for specification

Désignation
barres 120 x 10
longueur 2,40 m, étamé
185Power
185mm-System

Normes
IEC 61439-1:2011

Approbations
UL

Charactéristiques électriques
power dissipation at full load of the item:	174,0 W

Charactéristiques des matériaux
Embase:
	Cu-ETP R300 (EN 13601), tinned

corrosion-resistant, also in aggressive environments

Miscellaneous 
Tin-plated Cu busbars considerably reduce the effort of preparing the contact points.
The Cu busbars are effective protected against aggressive media.

Brand 
Woehner or equivalent

Référence
01767000