Text for specification

Descrizione
MIEZ
Multifunctional measuring device for front panel installation
Measurement of current, voltage, power, energy and derived values

Norme

Valori elettrici
tensione nominale (IEC) AC:	24 V
tensione nominale (IEC) DC:	24 V

power dissipation at full load of the item:	4.0 W
tensione max. ammissibile (IEC) AC:	50 V
tensione max. ammissibile (IEC) DC:	75 V

Brand 
Woehner or equivalent

Cod. art.
37002000A