Text for specification

Descrizione
MIEZ
Power analyser for front panel installation
Measurement of current, voltage, power, energy and derived values
Analysis and monitoring of voltage and power quality

Norme
EN 61010-1:2011 + A1
EN 61010-2-030:2011 + O1 + Z1

Valori elettrici
tensione nominale (IEC) AC:	24 V
tensione nominale (IEC) DC:	24 V

power dissipation at full load of the item:	4,0 W
tensione max. ammissibile (IEC) AC:	50 V
tensione max. ammissibile (IEC) DC:	75 V

Brand 
Woehner or equivalent

Cod. art.
37010000A